**Granit 1980i Industrial-Grade Full-Range Scanner Accessories**

|  |  |  |
| --- | --- | --- |
| **TYPE** | **SKU** | **DESCRIPTION** |
| Stand | STND-33F00-012-4 | gray, 33cm (13") height, flexible rod, weighted base, Granit cup |
| Stand | STND-30R00-011-4 | gray, 30cm (12") height, rigid rod, weighted base, Granit cradle |
| Holder | HOLDER-010-U | desktop/wall mount (include mounting hardware) |
| Vehicle Mount Kit | VMHOLDERK | contains vehicle mount forked holder (VM Holder), adjustable arm with ball joints (ADJARME) and mounting hardware |
| Cable | CBL-020-300-C00-01 | RS232 (5V signals), black, DB9 Female, 3m (9.8ft), coiled, 5V external power with option for host power on pin 9, industrial grade |
| Cable | CBL-500-300-S00-01 | USB, black, Type A, 3m (9.8'), straight, 5v host power, industrial grade |
| Cable | CBL-020-300-C00 | RS232 (5V signals), black, DB9 Female, 3m (9.8ft), coiled, 5V external power with option for host power on pin 9 |
| Cable | CBL-500-300-S00 | USB, black, Type A, 3m (9.8´), straight, 5V host power |
| Cable | CBL-500-300-C00 | USB, black, Type A, 3m (9.8´), coiled, 5V host power |
| Scanner heater with cable retractor | 520L-12-S3 | 12V, works with 8500 and Granit series of scanners |
| Scanner heater with cable retractor | 520L-24-S3 | 24V, works with 8500 and Granit series of scanners |
| Scanner heater with cable retractor | 520L-3648-S3 | 36-48V, works with 8500 and Granit series of scanners |
| Scanner heater | 521L-12-S3 | 12V, works with 8500 and Granit series of scanners |
| Scanner heater | 521L-24-S3 | 24V, works with 8500 and Granit series of scanners |
| Scanner heater | 521L-3648-S3 | 36-48V, works with 8500 and Granit seri |