**Granit 1980i Industrial-Grade Full-Range Scanner Accessories**

|  |  |  |
| --- | --- | --- |
| **TYPE**  | **SKU**  | **DESCRIPTION**  |
| Stand  | STND-33F00-012-4  | gray, 33cm (13") height, flexible rod, weighted base, Granit cup  |
| Stand  | STND-30R00-011-4  | gray, 30cm (12") height, rigid rod, weighted base, Granit cradle  |
| Holder  | HOLDER-010-U  | desktop/wall mount (include mounting hardware)  |
| Vehicle Mount Kit  | VMHOLDERK  | contains vehicle mount forked holder (VM Holder), adjustable arm with ball joints (ADJARME) and mounting hardware  |
| Cable  | CBL-020-300-C00-01  | RS232 (5V signals), black, DB9 Female, 3m (9.8ft), coiled, 5V external power with option for host power on pin 9, industrial grade  |
| Cable  | CBL-500-300-S00-01  | USB, black, Type A, 3m (9.8'), straight, 5v host power, industrial grade  |
| Cable  | CBL-020-300-C00  | RS232 (5V signals), black, DB9 Female, 3m (9.8ft), coiled, 5V external power with option for host power on pin 9  |
| Cable  | CBL-500-300-S00  | USB, black, Type A, 3m (9.8´), straight, 5V host power  |
| Cable  | CBL-500-300-C00  | USB, black, Type A, 3m (9.8´), coiled, 5V host power  |
| Scanner heater with cable retractor  | 520L-12-S3  | 12V, works with 8500 and Granit series of scanners  |
| Scanner heater with cable retractor  | 520L-24-S3  | 24V, works with 8500 and Granit series of scanners  |
| Scanner heater with cable retractor  | 520L-3648-S3  | 36-48V, works with 8500 and Granit series of scanners  |
| Scanner heater  | 521L-12-S3  | 12V, works with 8500 and Granit series of scanners  |
| Scanner heater  | 521L-24-S3  | 24V, works with 8500 and Granit series of scanners  |
| Scanner heater  | 521L-3648-S3  | 36-48V, works with 8500 and Granit seri |