**Granit 1981i Wireless Industrial-Grade Full-Range Scanner Accessories**

|  |  |  |
| --- | --- | --- |
| **TYPE**  | **SKU**  | **DESCRIPTION**  |
| Stand  | STND-33F00-012-4  | gray, 33cm (13") height, flexible rod, weighted base, Granit cup  |
| Stand  | STND-30R00-011-4  | gray, 30cm (12") height, rigid rod, weighted base, Granit cradle  |
| Holder  | HOLDER-010-U  | desktop/wall mount (include mounting hardware)  |
| Vehicle Mount Kit  | VMHOLDERK  | contains vehicle mount forked holder (VM Holder), adjustable arm with ball joints (ADJARME) and mounting hardware  |
| Access Point  | AP05-100BT-07N  | Granit 1981i, Class 1 Bluetooth, 100m (300'), up to 7 scanners can be connected RS232/USB/KBW (cables sold separately)  |
| Charge-Only Base  | COB02  | only 1 scanner can be charged at a time, power supply must be purchased separately  |
| Base  | CCB05-100BT-07N  | Granit 1981i, charging, Class 1 Bluetooth, 100m (300'), up to 7 scanners can be connected, RS232/USB/KBW host interfaces (cable sold separately)  |
| Cable  | CBL-020-300-C00-01  | RS232 (5V signals), black, DB9 Female, 3m (9.8ft), coiled, 5V external power with option for host power on pin 9, industrial grade  |
| Cable  | CBL-500-300-S00-01  | USB, black, Type A, 3m (9.8'), straight, 5v host power, industrial grade  |
| Cable  | CBL-020-300-C00  | RS232 (5V signals), black, DB9 Female, 3m (9.8ft), coiled, 5V external power with option for host power on pin 9  |
| Cable  | CBL-500-300-S00  | USB, black, Type A, 3m (9.8´), straight, 5V host power  |
| Cable  | CBL-500-300-C00  | USB, black, Type A, 3m (9.8´), coiled, 5V host power  |
| Battery  | BAT-SCN01  | Lithium-ion battery for Voyager 1202, Xenon 1902, Granit 1911i, 3820, 3820i, 4820, and 4820i cordless scanners  |
| Charger  | MB4-BAT-SCN01NAW0  | 4-bay battery charger (NA) for use with Voyager 1202g, Xenon 1902, Granit 1911i, Granit 1981i, 3820, 3820i, 4820 and 4820i Lithium-ion batteries, NA wallmount power supply (PS-050-4000W-NA), two mounting screws (100006897), and Instructions (MBC-INST)  |
| Charger  | MB4-BAT-SCN01NADO  | 4-bay battery charger (NA) for use with Voyager 1202g, Xenon 1902, Granit 1911i, Granit 1981i, 3820, 3820i, 4820 & 4820i Lithium-ion batteries, NA desktop power supply (PS-050-4000D-NA), two mounting screws (100006897), and Instructions (MBC-INST)  |
| Power Supply  | PS-05-1000W-A  | NA Plug, 1.0 A, 5.2VDC, 90  |
| Scanner heater with cable retractor  | 520L-12-S3  | 12V, works with 8500 and Granit series of scanners  |
| Scanner heater with cable retractor  | 520L-24-S3  | 24V, works with 8500 and Granit series of scanners  |
| Scanner heater with cable retractor  | 520L-3648-S3  | 36-48V, works with 8500 and Granit series of scanners  |
| Scanner heater  | 521L-12-S3  | 12V, works with 8500 and Granit series of scanners  |
| Scanner heater  | 521L-24-S3  | 24V, works with 8500 and Granit series of scanners  |
| Scanner heater  | 521L-3648-S3  | 36-48V, works with 8500 and Granit series of scanners  |
| Miscellaneous  | TOOLBAL  | Take up reel/balancer  |
|  | HOLSTER-INDUSTRIAL  | When clipped to a user's belt holster enables storage of Granit 1911i or Granit 1981i cordless scanner while leaving hands-free to accomplish other tasks (scanner sold separately)  |