**Granit 1981i Wireless Industrial-Grade Full-Range Scanner Accessories**

|  |  |  |
| --- | --- | --- |
| **TYPE** | **SKU** | **DESCRIPTION** |
| Stand | STND-33F00-012-4 | gray, 33cm (13") height, flexible rod, weighted base, Granit cup |
| Stand | STND-30R00-011-4 | gray, 30cm (12") height, rigid rod, weighted base, Granit cradle |
| Holder | HOLDER-010-U | desktop/wall mount (include mounting hardware) |
| Vehicle Mount Kit | VMHOLDERK | contains vehicle mount forked holder (VM Holder), adjustable arm with ball joints (ADJARME) and mounting hardware |
| Access Point | AP05-100BT-07N | Granit 1981i, Class 1 Bluetooth, 100m (300'), up to 7 scanners can be connected RS232/USB/KBW (cables sold separately) |
| Charge-Only Base | COB02 | only 1 scanner can be charged at a time, power supply must be purchased separately |
| Base | CCB05-100BT-07N | Granit 1981i, charging, Class 1 Bluetooth, 100m (300'), up to 7 scanners can be connected, RS232/USB/KBW host interfaces (cable sold separately) |
| Cable | CBL-020-300-C00-01 | RS232 (5V signals), black, DB9 Female, 3m (9.8ft), coiled, 5V external power with option for host power on pin 9, industrial grade |
| Cable | CBL-500-300-S00-01 | USB, black, Type A, 3m (9.8'), straight, 5v host power, industrial grade |
| Cable | CBL-020-300-C00 | RS232 (5V signals), black, DB9 Female, 3m (9.8ft), coiled, 5V external power with option for host power on pin 9 |
| Cable | CBL-500-300-S00 | USB, black, Type A, 3m (9.8´), straight, 5V host power |
| Cable | CBL-500-300-C00 | USB, black, Type A, 3m (9.8´), coiled, 5V host power |
| Battery | BAT-SCN01 | Lithium-ion battery for Voyager 1202, Xenon 1902, Granit 1911i, 3820, 3820i, 4820, and 4820i cordless scanners |
| Charger | MB4-BAT-SCN01NAW0 | 4-bay battery charger (NA) for use with Voyager 1202g, Xenon 1902, Granit 1911i, Granit 1981i, 3820, 3820i, 4820 and 4820i Lithium-ion batteries, NA wallmount power supply (PS-050-4000W-NA), two mounting screws (100006897), and Instructions (MBC-INST) |
| Charger | MB4-BAT-SCN01NADO | 4-bay battery charger (NA) for use with Voyager 1202g, Xenon 1902, Granit 1911i, Granit 1981i, 3820, 3820i, 4820 & 4820i Lithium-ion batteries, NA desktop power supply (PS-050-4000D-NA), two mounting screws (100006897), and Instructions (MBC-INST) |
| Power Supply | PS-05-1000W-A | NA Plug, 1.0 A, 5.2VDC, 90 |
| Scanner heater with cable retractor | 520L-12-S3 | 12V, works with 8500 and Granit series of scanners |
| Scanner heater with cable retractor | 520L-24-S3 | 24V, works with 8500 and Granit series of scanners |
| Scanner heater with cable retractor | 520L-3648-S3 | 36-48V, works with 8500 and Granit series of scanners |
| Scanner heater | 521L-12-S3 | 12V, works with 8500 and Granit series of scanners |
| Scanner heater | 521L-24-S3 | 24V, works with 8500 and Granit series of scanners |
| Scanner heater | 521L-3648-S3 | 36-48V, works with 8500 and Granit series of scanners |
| Miscellaneous | TOOLBAL | Take up reel/balancer |
|  | HOLSTER-INDUSTRIAL | When clipped to a user's belt holster enables storage of Granit 1911i or Granit 1981i cordless scanner while leaving hands-free to accomplish other tasks (scanner sold separately) |