**Voyager 1450g Upgradeable Area-Imaging Scanner Accessories**

|  |  |  |
| --- | --- | --- |
| **TYPE**  | **SKU**  | **DESCRIPTION**  |
| Power Supply  | 46-00525 STK  | NA plug, 1.0A @ 5.2VDC, 90-255VAC @ 50-60Hz  |
| Cable  | CBL-020-300-C00  | RS232 (5V signals), black, DB9 Female, 3m (9.8'), coiled, 5V external power with option for host power on pin 9  |
| Cable  | CBL-120-300-C00  | RS232C (+/-12V signals), black, DB9 Female, 3m (9.8'), coiled, 5V external power with option for host power on pin 9  |
| Cable  | CBL-220-300-C00  | RS232 (+5V signals), black, DB9 Male, 3m (9.8'), coiled, external power with option for host power on pin 9 for connection to Wincor Beetle  |
| Cable  | CBL-420-300-C00  | RS232 (5V signals), Honeywell Bioptic Stratos Aux, black, 10 pin modular, 3m (9.8'), coiled, host power possible (dependent upon scanner and Stratos models)  |
| STK Cable  | CBL-500-300-C00  | USB, black, Type A, 3m (9.8'), coiled, 5V host power  |
| STK Cable  | CBL-500-300-S00  | USB, black, Type A, 3m (9.8'), straight, 5V host power  |
| STK Cable  | CBL-500-500-C00  | USB, black, Type A, 5m (16.4'), coiled, 5V host power  |
| STK Cable  | CBL-503-300-C00  | USB, black, 12V locking, 3m (9.8'), coiled, 5V host power  |
| STK Cable  | CBL-600-400-C00  | IBM 46xx Port 9b, 12V Power, coiled, 4m (13.1')  |
| STK Cable  | CBL-720-300-C00  | KBW, black, PS2, 3m (9.8'), coiled, 5 V external power with option for host power  |
| STK Stand  | STND-15F03-009-4  | gray, 15cm (6") flexible rod, weighted mid-sized universal base, Voyager 1250 cup  |
| STD Holder  | HOLDER-009-U  | Universal holder (desk or wall)  |